This will need to be tested on your camera and alternations may need to be made. The last thing you guys will need is to integrate the *shape\_list* with ros subscriber to send (x,y) data and color to BBB for controller use

Version Control:

Cody Torno Date:12/9/2017

- Uploaded Pub.py and mv.py to google team drive (mv =machine vision).